
===============================

Default 3D printing parameters.
Nozzle 0.4mm
Layer height 0.2mm

===============================
BambooFeeder-AS1 Parts list: 
SG92R (or body size and arm size compatible model,  use the first hole of the servo arm), 13* FA2X8 self-tapping screws, 2* PB2X5/PM2X5 screws, 2* M3 hex nuts, 1+ * Oring-OD13*1mm, 1* spring 0.5*5*25

To assemble the AS1, rotate the servo to the 180 degree position first, simple method: 
After connecting the PPA1 machine normally, the feeder controller will also be enabled, connect the servo to any free feeder controller port and the servo will move to the desired angle.

If you have an 0816 controller or similar mathod for control, the reference for parameter setting is:
M620 N0 A180 B125 C55 F4 U500 V500 W2500 X1

Assembly reference£º
https://www.youtube.com/watch?v=DPH9m5KjhNc


===============================

License: CC BY-NC-SA 4.0
pandaplacer.com