=============================
20251212:
1. Repaired the PPBF-AS2-24-V1.1-All_PLA-PETG-ABS.3mf file error.
2. Remove MountingBlockA from .3mf. MountingBlockA using PETG/ABS.
20250908
=============================
Choose of print material:
# PLA/PETG/ABS/:
PPBF-AS2-**-V1.0-All*.3mf

# PETG/ABS:
PPBF-AS2-TopSpring-V1.0.STL
PPBF-AS2-TopClampingPlate_**-V1.0.STL
PPBF-AS2-MountingBlockA_**-V2.0.STL

Choose the color of the material:
Preferably with both black and white color difference, which is compatible with white, black, and clear tapes.
e.g. green, blue, yellow, orange...

* Some edges of the parts are pre-added with BRIM, please use a tool to remove the birm before assembly.
=============================

Assembly Notes:
1. Before inserting the SERVO, adjust the SERVO-Arm a bit towards to the retraction direction.
2. Using 2 O-rings on the spool and the friction is just right. More can be used when needed.
3. The mounting position needs to be aligned with the pin heads of the feeder controllers.

=============================

=============================



License: CC BY-NC-SA 4.0

Pandaplacer.com