Version V2.0 supports 6 Tips per Station.

Assembly:
Use 4-6 M2X8 self-tapping screws to secure the base and top.

assist_cap: 
This tool is used for alignment when setting nozzle Tip coordinates. For X Y coordinates, align the nozzle tip to the center of the crosshair.